Figure 8: Probability of Blocking vs load for varying number of timeslots05101520253035400.10.30.50.70.91.11.31.51.71.91/(avg interarrival time)

% Blocked

4 timeslots

6 timeslots

8 timeslots

10 timeslots

12 timeslots

Figure 9: Probability of Dropping vs load for varying number of timeslots0510152025303540450.10.30.50.70.91.11.31.51.71.91/(avg interarrival time)

% Dropped

Figure 6: Probability of Blocking vs load for varying maximum velocity01234567890.10.30.50.70.91.11.31.51.71.91/(avg interarrival time) vmax 100mph vmax 75 mph vmax 50 mph vmax 25 mph d(phi)max9.42 rad/s

Figure 7: Probability of Dropping vs load for varying maximum velocity05101520250.10.30.50.70.91.11.31.51.71.91/(avg interarrival time)